B51空中鼠标学习型遥控器
使用说明书

一．直接进入设备使用。

直接按设备键（如TVI,DVD等按键），可直接进入设备控制状态。

Enter into the device control status

Press the device button (such button of TVI,DVD),Can directly into  Enter into the device control status

二．手动搜索。

Search by manual

（1）、按下“SET”键3秒钟，直至LED灯亮后放开，然后按一下设备键（例如TV1、DVD

·····），LED闪烁一下，设备选择成功，若不选择设备，则默认为当前设备。
（1）、Press “SET” for 3 seconds until LED on, than press the device keyboard (such TV1、DVD….),the device have 

Success selected if the Led Shine.If not select device,  it will be select default device

（2）、按一下“CH+”或“POWER”键，每按一次，代码加1并发射“MUTE”或“PAUSE”

码；按一下“CH-”键，每按一次，代码减1并发射“MUTE”或“PAUSE”码；（在TV、CBL、SAT设备下显示“MUTE”符号，在VCR、DVD、CD、DVR、AUDIO下将显示“PAUSE”符号
（2）、Press “CH+” or “POWER”,the code will add 1 and send signal of “MUTE”or “PAUSE”when press one time,Press “CH-,the code will reduce 1 and send signal of “MUTE”or “PAUSE”when press one time,.

(The “Mute ” Sig will show when under the  device of TV、CBL、SAT ,and the “PAUSE” will show when under the device of VCR、DVD、CD、DVR、AUDIO
；

（3）、当搜索到当前设备可被遥控后，此时可以进一步按下其他按键进行测试；

     When the selected device is available for  control,  you can  go head testing by press other keys
（4）、若均能正确遥控，按一下“ENT”键保存并退出，此时LED熄灭；

     If every keyboard can be controlled ,presee the “ENG” to save  and exit, the LED will Off.

（5）、在搜索状态下，按下“SET”键或任意设备键，LED闪烁8次后将不保存退出；

      Under the  searching status , Press “SET” keyboard or any keyboard, It will not store when LED shining 8 times.

（6）、当搜索完成后，该设备下存储的所有学习键码将被全部删除。
 When searching is finished, all learning keyboard will be deleted 

三．自动搜索。

  AUTO-SEARCHING

（1）、按下“SET”键3秒钟，直至LED灯亮后放开，然后按一下设备键（例如TV1、DVD

·····），LED闪烁一下，设备选择成功，若不选择设备，则默认为当前设备。

(1). Press “SET” for 3 seconds until LED on, than press the device keyboard (such TV1、DVD….),the device have 

Success selected if the Led Shine If not select device,  it will be select default device,
（2）、按一下“CH+”、 “CH-”或“POWER”键，发射搜索码，进入搜索状态，若设备响应（在TV、CBL、SAT设备下显示“MUTE”符号，在VCR、DVD、CD、DVR、AUDIO下将显示“PAUSE”符号），按下其他按键进行测试，若正确，按“ENT”键保存并退出；不正确，则重新执行本步骤；

Press “CH+”“CH-”or “POWER” to send the search code to enter the searching status .if there is response from 

Device(The “Mute ” Sig will show when under the  device of TV、CBL、SA, “PAUSE” will show when under the device of VCR、DVD、CD、DVR、AUDIO), you can  go head testing by press other keys. If right ,press “ENT” to save and exit ;if wrong, do this step again.
)

（3）、等待3S以后，进入自动搜索；
      Waiting for 3S second to enter AUTO-SEARCH

（4）、等到设备响应，按任意键停止搜索；

     Press any key to stop search when device reponse

（5）、按下其他按键测试：To test by pressing  other keys

     A、测试正确，按“ENT”键保存并退出；If right ,pls to save and exit
     B、若不正确，估计是按键延时错过了能控制的码组，此时可按“CH-”进行递减搜索

（每按一次，发射VOL-/PLAY的码值），直到发现设备能被控制为止；

If wrong, it is may from  the delay of keyboard loss the control time of code-batch,you can  press “CH-”to continue

The degression searching(the  code value of VOL-/PLAY  will send for every press ) until device can be selected

（6）、在自动搜索设置过程中，任何时候按一下SAT或设备键，则LED灯闪8次后退出 。
      During the  Auto-searching  ,Press the key of SAT or device keyboard at any time , the LED will shine 8 time exit

（7）、当搜索完成后，该设备下存储的所有学习键码将被全部删除。

When searching is finished, all learning keyboard will be deleted

（8）、进入搜索状态后，自动搜索和手动搜索可以自由切换。
The  Auto-searching and  Manual searching can be  switch freely when entering the searching status.

四．学习功能

Learning Function 

（1）、按下“SET”键3秒钟，直至LED灯亮后放开，然后按一下设备键（例如TV1、DVD

·····），LED闪烁一下，设备选择成功，若不选择设备，则默认为当前设备。

Press “SET” for 3 seconds until LED on, than press the device keyboard (such TV1、DVD….),the device have 

Success selected if the Led Shine.If not select device,  it will be select default device

（2）、按一下“LEARNING”键，LED灯闪烁一下，进入学习状态；

 Pressing the Key of “LEARNING”,LED will shine to enter the  learning status.

（3）、将原遥控器的发射头对准本机接收头，距离约1~3厘米，按下需学习的按键约1秒；

若本机LED不停闪烁，表明学习成功，否则需重新学习；
Aim the  former  sender side of remote at our  remote, distance will be  1—3cm. Press  1 second

for the key you need learning. If new remote shining continually ,that mean learning second or need re-learning

（4）、按一下本机遥控器上要存储的按键，存下原始遥控器上发射的信号，LED恢复常亮，
进入下一次学习状态；

Press the key that need learning ,it will be store the signal from former key, LED return constant on ,go to next 

Learning status.

（5）、若完成学习，按一下“LEARNING”， LED熄灭，退出学习。
 If learning finished,press “Learning ”,LED Turn off ,exit learning

五．学习的删除。

Delete learning

（1）、按下“SET”键3秒钟，直至LED灯亮后放开，然后按一下设备键（例如TV1、DVD

·····），LED闪烁一下，设备选择成功，若不选择设备，则默认为当前设备。

Press “SET” for 3 seconds until LED on, than press the device keyboard (such TV1、DVD….),the device have 

Success selected if the Led Shine .If not select device,  it will be select default device

（2）、删除当前设备的某几个已学习键，输入特殊代码9919，LED闪一下后进入单键删除状态；

Input the special code of 9919 to delete the learned key, the per key delete status enter in when LED shine one time

（3）、按一下所需删除的按键，LED闪烁一下表示删除成功；若所按的键没有学习过，LED

闪烁3下表示删除失败。

Press the key which need delete ,it success when LED shine one time. If the key not  learning ,LED will shine 3 times ,fail to delete

（4）、按一下“LEARNING”， LED灯灭退出。

 Press “Learning key”, Led Off ,exit.
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